FILES
-----
GBR/IST-A35_PSS.PHO	SILKSCREEN PRIMARY              
GBR/IST-A35_PSM.PHO	SOLDER MASK PRIMARY             
GBR/IST-A35_PRI.PHO	PRIMARY LAYER                   
GBR/IST-A35_L02.PHO	LAYER 2                         
GBR/IST-A35_L03.PHO	LAYER 3                         
GBR/IST-A35_SEC.PHO	SECONDARY LAYER                 
GBR/IST-A35_SSM.PHO	SOLDER MASK SECONDARY           
GBR/IST-A35_SSS.PHO	SILKSCREEN SECONDARY            
GBR/IST-A35_PSP.PHO	PASTE MASK PRIMARY              
GBR/IST-A35_BRD.PHO	BOARD OUTLINE                   
GBR/IST-A35_FAB.PHO	FAB DRAWING                     
GBR/IST-A35_APR.REP	APERTURE FILE                   
GBR/IST-A35_NC.DRL	NC DRILL FILE                   
GBR/IST-A35_NC.REP	NC DRILL TOOLS                  
GBR/IST-A35_NET.IPC	IPC-D-356 NETLIST               
IST-A35.asc		PADS ASCII export file
IST-A35.dsn		Cadence schematic file
IST-A35.pcb		PADS PCB file
IST-A35-BOM.pdf		Bill of materials
IST-A35-GBR.pdf		Gerber files
IST-A35-SCH.pdf		Schematics
IST-A35-XY.xls 		Component coordinate + orientation chart

TECHNOLOGY
----------
4-LAYER
MINIMUM TRACE/SPACE: 5/5 (mils)
MINIMUM SMD PITCH: 0.5mm
SMD PAD COUNT:
PRI: 154
SEC: 0

GERBER FILE FORMAT
------------------
RS-274-X
2.5
ENGLISH
ABSOLUTE
TRAILING ZEROS SUPPRESSED


VENDOR MARKINGS
---------------
*** NO ADDED ETCH ALLOWED ***
SILKSCREEN ONLY




