FILES
-----
GBR/IST-A36_PSS.PHO	SILKSCREEN PRIMARY              
GBR/IST-A36_PSM.PHO	SOLDER MASK PRIMARY             
GBR/IST-A36_PRI.PHO	PRIMARY LAYER                   
GBR/IST-A36_SEC.PHO	SECONDARY LAYER                 
GBR/IST-A36_SSM.PHO	SOLDER MASK SECONDARY           
GBR/IST-A36_SSS.PHO	SILKSCREEN SECONDARY            
GBR/IST-A36_BRD.PHO	BOARD OUTLINE                   
GBR/IST-A36_FAB.PHO	FAB DRAWING                     
GBR/IST-A36_APR.REP	APERTURE FILE                   
GBR/IST-A36_NC.DRL	NC DRILL FILE                   
GBR/IST-A36_NC.REP	NC DRILL TOOLS                  
GBR/IST-A36_NET.IPC	IPC-D-356 NETLIST               
IST-A36.asc		PADS ASCII export file
IST-A36.dsn		Cadence schematic file
IST-A36.pcb		PADS PCB file
IST-A36-BOM.pdf		Bill of materials
IST-A36-GBR.pdf		Gerber files
IST-A36-SCH.pdf		Schematics

TECHNOLOGY
-----
2-LAYER
MINIMUM TRACE/SPACE: 12/7 (mils)
MINIMUM SMD PITCH: N/A
SMD PAD COUNT:
PRI: 0
SEC: 0

GERBER FILE FORMAT
-----
RS-274-X
2.4
ENGLISH
ABSOLUTE
TRAILING ZEROS SUPPRESSED

VENDOR MARKINGS
---------------
*** NO ADDED ETCH ALLOWED ***
SILKSCREEN ONLY



