| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros | Enumerations | Functions | Variables
Endpoint_UC3.h File Reference

USB Endpoint definitions for the AVR32 UC3 microcontrollers. More...

`#include "../../../../Common/Common.h"`
`#include "../USBTask.h"`
`#include "../USBInterrupt.h"`

## Macros
#define | ENDPOINT_CONTROLEP_DEFAULT_SIZE 8
#define | ENDPOINT_TOTAL_ENDPOINTS 7

## Enumerations
enum | Endpoint_WaitUntilReady_ErrorCodes_t { ENDPOINT_READYWAIT_NoError = 0, ENDPOINT_READYWAIT_EndpointStalled = 1, ENDPOINT_READYWAIT_DeviceDisconnected = 2, ENDPOINT_READYWAIT_BusSuspended = 3, ENDPOINT_READYWAIT_Timeout = 4, ENDPOINT_READYWAIT_NoError = 0, ENDPOINT_READYWAIT_EndpointStalled = 1, ENDPOINT_READYWAIT_DeviceDisconnected = 2, ENDPOINT_READYWAIT_BusSuspended = 3, ENDPOINT_READYWAIT_Timeout = 4, ENDPOINT_READYWAIT_NoError = 0, ENDPOINT_READYWAIT_EndpointStalled = 1, ENDPOINT_READYWAIT_DeviceDisconnected = 2, ENDPOINT_READYWAIT_BusSuspended = 3, ENDPOINT_READYWAIT_Timeout = 4, ENDPOINT_READYWAIT_NoError = 0, ENDPOINT_READYWAIT_EndpointStalled = 1, ENDPOINT_READYWAIT_DeviceDisconnected = 2, ENDPOINT_READYWAIT_BusSuspended = 3, ENDPOINT_READYWAIT_Timeout = 4 }

## Functions
static void | Endpoint_AbortPendingIN (void)
static uint16_t | Endpoint_BytesInEndpoint (void) ATTR_WARN_UNUSED_RESULT ATTR_ALWAYS_INLINE
static void | Endpoint_ClearIN (void) ATTR_ALWAYS_INLINE
static void | Endpoint_ClearOUT (void) ATTR_ALWAYS_INLINE
static void | Endpoint_ClearSETUP (void) ATTR_ALWAYS_INLINE
static void | Endpoint_ClearStall (void) ATTR_ALWAYS_INLINE
void | Endpoint_ClearStatusStage (void)
static bool | Endpoint_ConfigureEndpoint (const uint8_t Address, const uint8_t Type, const uint16_t Size, const uint8_t Banks) ATTR_ALWAYS_INLINE
bool | Endpoint_ConfigureEndpointTable (const USB_Endpoint_Table_t *const Table, const uint8_t Entries)
static void | Endpoint_DisableEndpoint (void) ATTR_ALWAYS_INLINE
static void | Endpoint_Discard_16 (void) ATTR_ALWAYS_INLINE
static void | Endpoint_Discard_32 (void) ATTR_ALWAYS_INLINE
static void | Endpoint_Discard_8 (void) ATTR_ALWAYS_INLINE
static void | Endpoint_EnableEndpoint (void) ATTR_ALWAYS_INLINE
static uint8_t | Endpoint_GetBusyBanks (void) ATTR_ALWAYS_INLINE ATTR_WARN_UNUSED_RESULT
static uint8_t | Endpoint_GetCurrentEndpoint (void) ATTR_WARN_UNUSED_RESULT ATTR_ALWAYS_INLINE
static uint32_t | Endpoint_GetEndpointDirection (void) ATTR_WARN_UNUSED_RESULT ATTR_ALWAYS_INLINE
static uint32_t | Endpoint_GetEndpointInterrupts (void) ATTR_WARN_UNUSED_RESULT ATTR_ALWAYS_INLINE
static bool | Endpoint_HasEndpointInterrupted (const uint8_t Address) ATTR_WARN_UNUSED_RESULT ATTR_ALWAYS_INLINE
static bool | Endpoint_IsConfigured (void) ATTR_WARN_UNUSED_RESULT ATTR_ALWAYS_INLINE
static bool | Endpoint_IsEnabled (void) ATTR_WARN_UNUSED_RESULT ATTR_ALWAYS_INLINE
static bool | Endpoint_IsINReady (void) ATTR_WARN_UNUSED_RESULT ATTR_ALWAYS_INLINE
static bool | Endpoint_IsOUTReceived (void) ATTR_WARN_UNUSED_RESULT ATTR_ALWAYS_INLINE
static bool | Endpoint_IsReadWriteAllowed (void) ATTR_WARN_UNUSED_RESULT ATTR_ALWAYS_INLINE
static bool | Endpoint_IsSETUPReceived (void) ATTR_WARN_UNUSED_RESULT ATTR_ALWAYS_INLINE
static bool | Endpoint_IsStalled (void) ATTR_WARN_UNUSED_RESULT ATTR_ALWAYS_INLINE
static uint16_t | Endpoint_Read_16_BE (void) ATTR_WARN_UNUSED_RESULT ATTR_ALWAYS_INLINE
static uint16_t | Endpoint_Read_16_LE (void) ATTR_WARN_UNUSED_RESULT ATTR_ALWAYS_INLINE
static uint32_t | Endpoint_Read_32_BE (void) ATTR_WARN_UNUSED_RESULT ATTR_ALWAYS_INLINE
static uint32_t | Endpoint_Read_32_LE (void) ATTR_WARN_UNUSED_RESULT ATTR_ALWAYS_INLINE
static uint8_t | Endpoint_Read_8 (void) ATTR_WARN_UNUSED_RESULT ATTR_ALWAYS_INLINE
static void | Endpoint_ResetDataToggle (void) ATTR_ALWAYS_INLINE
static void | Endpoint_ResetEndpoint (const uint8_t Address) ATTR_ALWAYS_INLINE
static void | Endpoint_SelectEndpoint (const uint8_t Address) ATTR_ALWAYS_INLINE
static void | Endpoint_SetEndpointDirection (const uint32_t DirectionMask) ATTR_ALWAYS_INLINE
static void | Endpoint_StallTransaction (void) ATTR_ALWAYS_INLINE
uint8_t | Endpoint_WaitUntilReady (void)
static void | Endpoint_Write_16_BE (const uint16_t Data) ATTR_ALWAYS_INLINE
static void | Endpoint_Write_16_LE (const uint16_t Data) ATTR_ALWAYS_INLINE
static void | Endpoint_Write_32_BE (const uint32_t Data) ATTR_ALWAYS_INLINE
static void | Endpoint_Write_32_LE (const uint32_t Data) ATTR_ALWAYS_INLINE
static void | Endpoint_Write_8 (const uint8_t Data) ATTR_ALWAYS_INLINE

## Variables
uint8_t | USB_Device_ControlEndpointSize

## Detailed Description

Functions, macros and enums related to endpoint management when in USB Device mode. This module contains the endpoint management macros, as well as endpoint interrupt and data send/receive functions for various data types.

Note
  This file should not be included directly. It is automatically included as needed by the USB driver dispatch header located in LUFA/Drivers/USB/USB.h.