| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
USB_Descriptor_Endpoint_t Struct Reference
USB Descriptors

Standard USB Endpoint Descriptor (LUFA naming conventions). More...

`#include <StdDescriptors.h>`

## Data Fields
uint8_t | Attributes
uint8_t | EndpointAddress
uint16_t | EndpointSize
USB_Descriptor_Header_t | Header
uint8_t | PollingIntervalMS

## Detailed Description

Type define for a standard Endpoint Descriptor. This structure uses LUFA-specific element names to make each element's purpose clearer.

See also
  USB_StdDescriptor_Endpoint_t for the version of this type with standard element names.

Note
  Regardless of CPU architecture, these values should be stored as little endian.

## Field Documentation

uint8_t USB_Descriptor_Endpoint_t::Attributes

Endpoint attributes, comprised of a mask of the endpoint type (EP_TYPE_*) and attributes (ENDPOINT_ATTR_*) masks.

uint8_t USB_Descriptor_Endpoint_t::EndpointAddress

Logical address of the endpoint within the device for the current configuration, including direction mask.

uint16_t USB_Descriptor_Endpoint_t::EndpointSize

Size of the endpoint bank, in bytes. This indicates the maximum packet size that the endpoint can receive at a time.

USB_Descriptor_Header_t USB_Descriptor_Endpoint_t::Header

Descriptor header, including type and size.

uint8_t USB_Descriptor_Endpoint_t::PollingIntervalMS

Polling interval in milliseconds for the endpoint if it is an INTERRUPT or ISOCHRONOUS type.

The documentation for this struct was generated from the following file:

- Drivers/USB/Core/StdDescriptors.h