| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros
LEDs.h File Reference

Board specific LED driver header for the Xevelabs USB2AX. More...

`#include "../../../../Common/Common.h"`

## Macros
#define | LEDS_ALL_LEDS (LEDS_LED1 | LEDS_LED2)
#define | LEDS_LED1 USB2AX_LEDS_LED1
#define | LEDS_LED2 USB2AX_LEDS_LED2
#define | LEDS_NO_LEDS 0

## Detailed Description

Note
  For version 3 USB2AX boards, compile with `BOARD = USB2AX_V3` and for version 3.1, with `BOARD = USB2AX_V31`.

Board specific LED driver header for the Xevelabs USB2AX (http://paranoidstudio.assembla.com/wiki/show/paranoidstudio/USB2AX).

USB2AX:

Name | Color | Info | Active Level | Port Pin
--- | --- | --- | --- | ---
LEDS_LED1 | Green | General Indicator | High | PORTC.6

USB2AX_V3:

Name | Color | Info | Active Level | Port Pin
--- | --- | --- | --- | ---
LEDS_LED1 | Green | General Indicator | High | PORTD.1

USB2AX_V31:

Name | Color | Info | Active Level | Port Pin
--- | --- | --- | --- | ---
LEDS_LED1 | Green | General Indicator | High | PORTD.5
LEDS_LED2 | Red | General Indicator | High | PORTD.6

Note
  This file should not be included directly. It is automatically included as needed by the LEDs driver dispatch header located in LUFA/Drivers/Board/LEDs.h.