| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
SCSI_Request_Sense_Response_t Struct Reference
Common Class Definitions

Mass Storage Class SCSI Sense Structure. More...

`#include <MassStorageClassCommon.h>`

## Data Fields
uint8_t | AdditionalLength
uint8_t | AdditionalSenseCode
uint8_t | AdditionalSenseQualifier
uint8_t | CmdSpecificInformation [4]
unsigned | EOM: 1
uint8_t | FieldReplaceableUnitCode
unsigned | FileMark: 1
unsigned | ILI: 1
uint8_t | Information [4]
unsigned | Reserved: 1
uint8_t | ResponseCode
uint8_t | SegmentNumber
unsigned | SenseKey: 4
uint8_t | SenseKeySpecific [3]

## Detailed Description

Type define for a SCSI Sense structure. Structures of this type are filled out by the device via the MS_Host_RequestSense() function, indicating the current sense data of the device (giving explicit error codes for the last issued command). For details of the structure contents, refer to the SCSI specifications.

## Field Documentation

uint8_t SCSI_Request_Sense_Response_t::AdditionalLength

uint8_t SCSI_Request_Sense_Response_t::AdditionalSenseCode

uint8_t SCSI_Request_Sense_Response_t::AdditionalSenseQualifier

uint8_t SCSI_Request_Sense_Response_t::CmdSpecificInformation[4]

unsigned SCSI_Request_Sense_Response_t::EOM

uint8_t SCSI_Request_Sense_Response_t::FieldReplaceableUnitCode

unsigned SCSI_Request_Sense_Response_t::FileMark

unsigned SCSI_Request_Sense_Response_t::ILI

uint8_t SCSI_Request_Sense_Response_t::Information[4]

unsigned SCSI_Request_Sense_Response_t::Reserved

uint8_t SCSI_Request_Sense_Response_t::ResponseCode

uint8_t SCSI_Request_Sense_Response_t::SegmentNumber

unsigned SCSI_Request_Sense_Response_t::SenseKey

uint8_t SCSI_Request_Sense_Response_t::SenseKeySpecific[3]

The documentation for this struct was generated from the following file:

- Drivers/USB/Class/Common/MassStorageClassCommon.h