| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Modules | Data Structures | Macros
Pipe Management
USB Core - LUFA/Drivers/USB/USB.h

Pipe management definitions. More...

## Modules
| Pipe Control Request Management
| Pipe control request definitions.
| Pipe Data Reading and Writing
| Pipe data read/write definitions.
| Pipe Management (AVR8)
| Pipe management definitions for the Atmel AVR8 architecture.
| Pipe Management (UC3)
| Pipe management definitions for the Atmel AVR32 UC3 architecture.
| Pipe Packet Management
| Pipe packet management definitions.

## Data Structures
struct | USB_Pipe_Table_t

## Macros
#define | PIPE_CONTROLPIPE 0
#define | PIPE_EPNUM_MASK 0x0F
#define | PIPE_PIPENUM_MASK 0x0F

## Detailed Description

This module contains functions, macros and enums related to pipe management when in USB Host mode. This module contains the pipe management macros, as well as pipe interrupt and data send/receive functions for various data types.

## Macro Definition Documentation

#define PIPE_CONTROLPIPE 0

Pipe address for the default control pipe, which always resides in address 0. This is defined for convenience to give more readable code when used with the pipe macros.

#define PIPE_EPNUM_MASK 0x0F

Endpoint number mask, for masking against endpoint addresses to retrieve the endpoint's numerical address in the attached device.

#define PIPE_PIPENUM_MASK 0x0F

Pipe number mask, for masking against pipe addresses to retrieve the pipe's numerical address in the device.