| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros | Enumerations | Functions
Host_UC3.h File Reference

USB Host definitions for the AVR32 UC3B microcontrollers. More...

`#include "../../../../Common/Common.h"`
`#include "../StdDescriptors.h"`
`#include "../Pipe.h"`
`#include "../USBInterrupt.h"`

## Macros
#define | HOST_DEVICE_SETTLE_DELAY_MS 1000
#define | USB_HOST_DEVICEADDRESS 1

## Enumerations
enum | USB_Host_EnumerationErrorCodes_t { HOST_ENUMERROR_NoError = 0, HOST_ENUMERROR_WaitStage = 1, HOST_ENUMERROR_NoDeviceDetected = 2, HOST_ENUMERROR_ControlError = 3, HOST_ENUMERROR_PipeConfigError = 4, HOST_ENUMERROR_NoError = 0, HOST_ENUMERROR_WaitStage = 1, HOST_ENUMERROR_NoDeviceDetected = 2, HOST_ENUMERROR_ControlError = 3, HOST_ENUMERROR_PipeConfigError = 4 }
enum | USB_Host_ErrorCodes_t { HOST_ERROR_VBusVoltageDip = 0, HOST_ERROR_VBusVoltageDip = 0 }

## Functions
static void | USB_Host_ClearRemoteWakeupSent (void) ATTR_ALWAYS_INLINE
static void | USB_Host_DisableSOFEvents (void) ATTR_ALWAYS_INLINE
static void | USB_Host_EnableSOFEvents (void) ATTR_ALWAYS_INLINE
static uint16_t | USB_Host_GetFrameNumber (void) ATTR_WARN_UNUSED_RESULT ATTR_ALWAYS_INLINE
static bool | USB_Host_IsBusResetComplete (void) ATTR_WARN_UNUSED_RESULT ATTR_ALWAYS_INLINE
static bool | USB_Host_IsBusSuspended (void) ATTR_WARN_UNUSED_RESULT ATTR_ALWAYS_INLINE
static bool | USB_Host_IsDeviceFullSpeed (void) ATTR_WARN_UNUSED_RESULT ATTR_ALWAYS_INLINE
static bool | USB_Host_IsRemoteWakeupSent (void) ATTR_WARN_UNUSED_RESULT ATTR_ALWAYS_INLINE
static bool | USB_Host_IsResumeFromWakeupRequestSent (void) ATTR_WARN_UNUSED_RESULT ATTR_ALWAYS_INLINE
static void | USB_Host_ResetBus (void) ATTR_ALWAYS_INLINE
static void | USB_Host_ResumeBus (void) ATTR_ALWAYS_INLINE
static void | USB_Host_ResumeFromWakeupRequest (void) ATTR_ALWAYS_INLINE
static void | USB_Host_SuspendBus (void) ATTR_ALWAYS_INLINE

## Detailed Description

Architecture specific USB Host definitions for the Atmel 32-bit AVR UC3B microcontrollers.

Note
  This file should not be included directly. It is automatically included as needed by the USB driver dispatch header located in LUFA/Drivers/USB/USB.h.