| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
USB_StdDescriptor_Endpoint_t Struct Reference
USB Descriptors

Standard USB Endpoint Descriptor (USB-IF naming conventions). More...

`#include <StdDescriptors.h>`

## Data Fields
uint8_t | bDescriptorType
uint8_t | bEndpointAddress
uint8_t | bInterval
uint8_t | bLength
uint8_t | bmAttributes
uint16_t | wMaxPacketSize

## Detailed Description

Type define for a standard Endpoint Descriptor. This structure uses the relevant standard's given element names to ensure compatibility with the standard.

See also
  USB_Descriptor_Endpoint_t for the version of this type with non-standard LUFA specific element names.

Note
  Regardless of CPU architecture, these values should be stored as little endian.

## Field Documentation

uint8_t USB_StdDescriptor_Endpoint_t::bDescriptorType

Type of the descriptor, either a value in USB_DescriptorTypes_t or a value given by the specific class.

uint8_t USB_StdDescriptor_Endpoint_t::bEndpointAddress

Logical address of the endpoint within the device for the current configuration, including direction mask.

uint8_t USB_StdDescriptor_Endpoint_t::bInterval

Polling interval in milliseconds for the endpoint if it is an INTERRUPT or ISOCHRONOUS type.

uint8_t USB_StdDescriptor_Endpoint_t::bLength

Size of the descriptor, in bytes.

uint8_t USB_StdDescriptor_Endpoint_t::bmAttributes

Endpoint attributes, comprised of a mask of the endpoint type (EP_TYPE_*) and attributes (ENDPOINT_ATTR_*) masks.

uint16_t USB_StdDescriptor_Endpoint_t::wMaxPacketSize

Size of the endpoint bank, in bytes. This indicates the maximum packet size that the endpoint can receive at a time.

The documentation for this struct was generated from the following file:

- Drivers/USB/Core/StdDescriptors.h