| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
RNDIS_Reset_Complete_t Struct Reference
Common Class Definitions

RNDIS Reset Complete Message Structure. More...

`#include <RNDISClassCommon.h>`

## Data Fields
uint32_t | AddressingReset
uint32_t | MessageLength
uint32_t | MessageType
uint32_t | Status

## Detailed Description

Type define for a RNDIS Reset Complete response message.

Note
  Regardless of CPU architecture, these values should be stored as little endian.

## Field Documentation

uint32_t RNDIS_Reset_Complete_t::AddressingReset

uint32_t RNDIS_Reset_Complete_t::MessageLength

uint32_t RNDIS_Reset_Complete_t::MessageType

uint32_t RNDIS_Reset_Complete_t::Status

The documentation for this struct was generated from the following file:

- Drivers/USB/Class/Common/RNDISClassCommon.h