| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Structures | Macros | Enumerations
StdRequestType.h File Reference

USB control endpoint request definitions. More...

`#include "../../../Common/Common.h"`
`#include "USBMode.h"`

## Data Structures
struct | USB_Request_Header_t
| Standard USB Control Request. More...

## Macros
#define | CONTROL_REQTYPE_DIRECTION 0x80
#define | CONTROL_REQTYPE_RECIPIENT 0x1F
#define | CONTROL_REQTYPE_TYPE 0x60
Control Request Data Direction Masks
#define | REQDIR_HOSTTODEVICE (0 << 7)
#define | REQDIR_DEVICETOHOST (1 << 7)
Control Request Type Masks
#define | REQTYPE_STANDARD (0 << 5)
#define | REQTYPE_CLASS (1 << 5)
#define | REQTYPE_VENDOR (2 << 5)
Control Request Recipient Masks
#define | REQREC_DEVICE (0 << 0)
#define | REQREC_INTERFACE (1 << 0)
#define | REQREC_ENDPOINT (2 << 0)
#define | REQREC_OTHER (3 << 0)

## Enumerations
enum | USB_Control_Request_t { REQ_GetStatus = 0, REQ_ClearFeature = 1, REQ_SetFeature = 3, REQ_SetAddress = 5, REQ_GetDescriptor = 6, REQ_SetDescriptor = 7, REQ_GetConfiguration = 8, REQ_SetConfiguration = 9, REQ_GetInterface = 10, REQ_SetInterface = 11, REQ_SynchFrame = 12 }
enum | USB_Feature_Selectors_t { FEATURE_SEL_EndpointHalt = 0x00, FEATURE_SEL_DeviceRemoteWakeup = 0x01, FEATURE_SEL_TestMode = 0x02 }

## Detailed Description

This module contains definitions for the various control request parameters, so that the request details (such as data direction, request recipient, etc.) can be extracted via masking.

Note
  This file should not be included directly. It is automatically included as needed by the USB driver dispatch header located in LUFA/Drivers/USB/USB.h.