| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros
Dataflash.h File Reference

LUFA Custom Board Dataflash Hardware Driver (Template) More...

## Macros
#define | DATAFLASH_CHIP1
#define | DATAFLASH_CHIP2
#define | DATAFLASH_NO_CHIP 0
#define | DATAFLASH_PAGE_SIZE
#define | DATAFLASH_PAGES
#define | DATAFLASH_TOTALCHIPS 1

## Detailed Description

This is a stub driver header file, for implementing custom board layout hardware with compatible LUFA board specific drivers. If the library is configured to use the BOARD_USER board mode, this driver file should be completed and copied into the "/Board/" folder inside the application's folder.

This stub is for the board-specific component of the LUFA Dataflash driver.

## Macro Definition Documentation

#define DATAFLASH_CHIP1

Mask for the first dataflash chip selected.

#define DATAFLASH_CHIP2

Mask for the second dataflash chip selected.

#define DATAFLASH_NO_CHIP 0

Mask for no dataflash chip selected.

#define DATAFLASH_PAGE_SIZE

Internal main memory page size for the board's dataflash ICs.

#define DATAFLASH_PAGES

Total number of pages inside each of the board's dataflash ICs.

#define DATAFLASH_TOTALCHIPS 1

Constant indicating the total number of dataflash ICs mounted on the selected board.