| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros
STANGE_ISP
LEDs Driver - LUFA/Drivers/Board/LEDs.h

Board specific LED driver header for the Dimex Stange-ISP board. More...

## Macros
#define | LEDS_ALL_LEDS (LEDS_LED1 | LEDS_LED2)
#define | LEDS_LED1 (1 << 0)
#define | LEDS_LED2 (1 << 1)
#define | LEDS_NO_LEDS 0

## Detailed Description

Board specific LED driver header for the Dimex Stange-ISP board (http://www.diamex.de/dxshop/USB-ISP-Programmer-fuer-Atmel-AVR).

Name | Color | Info | Active Level | Port Pin
--- | --- | --- | --- | ---
LEDS_LED1 | Green | General Indicator | Low | PORTD.0
LEDS_LED2 | Red | General Indicator | Low | PORTD.1

## Macro Definition Documentation

#define LEDS_ALL_LEDS (LEDS_LED1 | LEDS_LED2)

LED mask for all the LEDs on the board.

#define LEDS_LED1 (1 << 0)

LED mask for the first LED on the board.

#define LEDS_LED2 (1 << 1)

LED mask for the second LED on the board.

#define LEDS_NO_LEDS 0

LED mask for none of the board LEDs.