| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros
EVK1101
LEDs Driver - LUFA/Drivers/Board/LEDs.h

Board specific LED driver header for the Atmel EVK1101. More...

## Macros
#define | LEDS_ALL_LEDS (LEDS_LED1 | LEDS_LED2 | LEDS_LED3 | LEDS_LED4)
#define | LEDS_LED1 (1UL << 7)
#define | LEDS_LED2 (1UL << 8)
#define | LEDS_LED3 (1UL << 21)
#define | LEDS_LED4 (1UL << 22)
#define | LEDS_NO_LEDS 0

## Detailed Description

Board specific LED driver header for the Atmel EVK1101.

Name | Color | Info | Active Level | Port Pin
--- | --- | --- | --- | ---
LEDS_LED1 | Green | LED0 LED | Low | GPIO7
LEDS_LED2 | Green | LED1 LED | Low | GPIO8
LEDS_LED3 | Green | LED2 LED | Low | GPIO21
LEDS_LED4 | Green | LED3 LED | Low | GPIO22

## Macro Definition Documentation

#define LEDS_ALL_LEDS (LEDS_LED1 | LEDS_LED2 | LEDS_LED3 | LEDS_LED4)

LED mask for all the LEDs on the board.

#define LEDS_LED1 (1UL << 7)

LED mask for the first LED on the board.

#define LEDS_LED2 (1UL << 8)

LED mask for the second LED on the board.

#define LEDS_LED3 (1UL << 21)

LED mask for the third LED on the board.

#define LEDS_LED4 (1UL << 22)

LED mask for the fourth LED on the board.

#define LEDS_NO_LEDS 0

LED mask for the none of the board LEDs