| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
RNDIS_Initialize_Complete_t Struct Reference
Common Class Definitions

RNDIS Initialize Complete Message Structure. More...

`#include <RNDISClassCommon.h>`

## Data Fields
uint32_t | AFListOffset
uint32_t | AFListSize
uint32_t | DeviceFlags
uint32_t | MajorVersion
uint32_t | MaxPacketsPerTransfer
uint32_t | MaxTransferSize
uint32_t | Medium
uint32_t | MessageLength
uint32_t | MessageType
uint32_t | MinorVersion
uint32_t | PacketAlignmentFactor
uint32_t | RequestId
uint32_t | Status

## Detailed Description

Type define for a RNDIS Initialize Complete response message.

Note
  Regardless of CPU architecture, these values should be stored as little endian.

## Field Documentation

uint32_t RNDIS_Initialize_Complete_t::AFListOffset

uint32_t RNDIS_Initialize_Complete_t::AFListSize

uint32_t RNDIS_Initialize_Complete_t::DeviceFlags

uint32_t RNDIS_Initialize_Complete_t::MajorVersion

uint32_t RNDIS_Initialize_Complete_t::MaxPacketsPerTransfer

uint32_t RNDIS_Initialize_Complete_t::MaxTransferSize

uint32_t RNDIS_Initialize_Complete_t::Medium

uint32_t RNDIS_Initialize_Complete_t::MessageLength

uint32_t RNDIS_Initialize_Complete_t::MessageType

uint32_t RNDIS_Initialize_Complete_t::MinorVersion

uint32_t RNDIS_Initialize_Complete_t::PacketAlignmentFactor

uint32_t RNDIS_Initialize_Complete_t::RequestId

uint32_t RNDIS_Initialize_Complete_t::Status

The documentation for this struct was generated from the following file:

- Drivers/USB/Class/Common/RNDISClassCommon.h