| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros
BIGMULTIO
LEDs Driver - LUFA/Drivers/Board/LEDs.h

Board specific LED driver header for the Bitwizard Big-Multio. More...

## Macros
#define | LEDS_ALL_LEDS (LEDS_LED1 | LEDS_LED2 | LEDS_LED3)
#define | LEDS_LED1 (1 << 6)
#define | LEDS_LED2 (1 << 7)
#define | LEDS_LED3 (1 << 2)
#define | LEDS_NO_LEDS 0

## Detailed Description

Board specific LED driver header for the Bitwizard Big-Multio (http://www.bitwizard.nl/wiki/index.php/Usbbigmultio).

Name | Color | Info | Active Level | Port Pin
--- | --- | --- | --- | ---
LEDS_LED1 | Unknown | LED0 | High | PORTF.6
LEDS_LED2 | Unknown | LED1 | High | PORTF.7
LEDS_LED3 | Unknown | LED2 | High | PORTE.2

## Macro Definition Documentation

#define LEDS_ALL_LEDS (LEDS_LED1 | LEDS_LED2 | LEDS_LED3)

LED mask for all the LEDs on the board.

#define LEDS_LED1 (1 << 6)

LED mask for the first LED on the board.

#define LEDS_LED2 (1 << 7)

LED mask for the second LED on the board.

#define LEDS_LED3 (1 << 2)

LED mask for the second LED on the board.

#define LEDS_NO_LEDS 0

LED mask for none of the board LEDs.