| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros
A3BU_XPLAINED
LEDs Driver - LUFA/Drivers/Board/LEDs.h

Board specific LED driver header for the Atmel XMEGA A3BU Xplained. More...

## Macros
#define | LEDS_ALL_LEDS (LEDS_LED1 | LEDS_LED2 | LEDS_LED3 | LEDS_LED4)
#define | LEDS_LED1 (1 << 0)
#define | LEDS_LED2 (1 << 1)
#define | LEDS_LED3 (1 << 4)
#define | LEDS_LED4 (1 << 5)
#define | LEDS_NO_LEDS 0

## Detailed Description

Board specific LED driver header for the Atmel XMEGA A3BU Xplained.

Name | Color | Info | Active Level | Port Pin
--- | --- | --- | --- | ---
LEDS_LED1 | Yellow | LED0 LED | Low | PORTR.0
LEDS_LED2 | Yellow | LED1 LED | Low | PORTR.1
LEDS_LED3 | Red | Status Bicolour Red LED | Low | PORTD.4
LEDS_LED4 | Green | Status Bicolour Green LED | High | PORTD.5

## Macro Definition Documentation

#define LEDS_ALL_LEDS (LEDS_LED1 | LEDS_LED2 | LEDS_LED3 | LEDS_LED4)

LED mask for all the LEDs on the board.

#define LEDS_LED1 (1 << 0)

LED mask for the first LED on the board.

#define LEDS_LED2 (1 << 1)

LED mask for the second LED on the board.

#define LEDS_LED3 (1 << 4)

LED mask for the third LED on the board.

#define LEDS_LED4 (1 << 5)

LED mask for the fourth LED on the board.

#define LEDS_NO_LEDS 0

LED mask for none of the board LEDs.