| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros
Joystick.h File Reference

Board specific joystick driver header for the Fletchtronics BUMBLEB. More...

`#include "../../../../Common/Common.h"`

## Macros
#define | JOY_DOWN (1 << 1)
#define | JOY_LEFT (1 << 2)
#define | JOY_PRESS (1 << 4)
#define | JOY_RIGHT (1 << 0)
#define | JOY_UP (1 << 3)

## Detailed Description

Board specific joystick driver header for the Fletchtronics BUMBLEB (http://fletchtronics.net/bumble-b). The BUMBLEB third-party board does not include any on-board peripherals, but does have an officially recommended external peripheral layout for buttons, LEDs and a Joystick.

Left Port Pin | Up Port Pin | Right Port Pin | Down Port Pin | Press Port Pin
--- | --- | --- | --- | ---
PORTD.2 | PORTD.3 | PORTD.0 | PORTD.1 | PORTD.4

Note
  This file should not be included directly. It is automatically included as needed by the joystick driver dispatch header located in LUFA/Drivers/Board/Joystick.h.