| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Structures | Functions
RNDISClassDevice.h File Reference

Device mode driver for the library USB RNDIS Class driver. More...

`#include "../../USB.h"`
`#include "../Common/RNDISClassCommon.h"`

## Data Structures
struct | USB_ClassInfo_RNDIS_Device_t
| RNDIS Class Device Mode Configuration and State Structure. More...

## Functions
bool | RNDIS_Device_ConfigureEndpoints (USB_ClassInfo_RNDIS_Device_t *const RNDISInterfaceInfo) ATTR_NON_NULL_PTR_ARG(1)
bool | RNDIS_Device_IsPacketReceived (USB_ClassInfo_RNDIS_Device_t *const RNDISInterfaceInfo) ATTR_NON_NULL_PTR_ARG(1)
void | RNDIS_Device_ProcessControlRequest (USB_ClassInfo_RNDIS_Device_t *const RNDISInterfaceInfo) ATTR_NON_NULL_PTR_ARG(1)
uint8_t | RNDIS_Device_ReadPacket (USB_ClassInfo_RNDIS_Device_t *const RNDISInterfaceInfo, void *Buffer, uint16_t *const PacketLength) ATTR_NON_NULL_PTR_ARG(1)
uint8_t | RNDIS_Device_SendPacket (USB_ClassInfo_RNDIS_Device_t *const RNDISInterfaceInfo, void *Buffer, const uint16_t PacketLength) ATTR_NON_NULL_PTR_ARG(1)
void | RNDIS_Device_USBTask (USB_ClassInfo_RNDIS_Device_t *const RNDISInterfaceInfo) ATTR_NON_NULL_PTR_ARG(1)

## Detailed Description

Device mode driver for the library USB RNDIS Class driver.

Note
  This file should not be included directly. It is automatically included as needed by the USB module driver dispatch header located in LUFA/Drivers/USB.h.