| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
USB_Audio_Descriptor_StreamEndpoint_Spc_t Struct Reference
Common Class Definitions

Audio class-specific Extended Endpoint Descriptor (LUFA naming conventions). More...

`#include <AudioClassCommon.h>`

## Data Fields
uint8_t | Attributes
USB_Descriptor_Header_t | Header
uint16_t | LockDelay
uint8_t | LockDelayUnits
uint8_t | Subtype

## Detailed Description

Type define for an Audio class-specific extended endpoint descriptor. This contains extra information on the usage of endpoints used to stream audio in and out of the USB Audio device, and follows an Audio class-specific extended endpoint descriptor. See the USB Audio specification for more details.

See also
  USB_Audio_StdDescriptor_StreamEndpoint_Spc_t for the version of this type with standard element names.

Note
  Regardless of CPU architecture, these values should be stored as little endian.

## Field Documentation

uint8_t USB_Audio_Descriptor_StreamEndpoint_Spc_t::Attributes

Audio class-specific endpoint attributes, such as AUDIO_EP_FULL_PACKETS_ONLY.

USB_Descriptor_Header_t USB_Audio_Descriptor_StreamEndpoint_Spc_t::Header

Regular descriptor header containing the descriptor's type and length.

uint16_t USB_Audio_Descriptor_StreamEndpoint_Spc_t::LockDelay

Time required to internally lock endpoint's internal clock recovery circuitry.

uint8_t USB_Audio_Descriptor_StreamEndpoint_Spc_t::LockDelayUnits

Units used for the LockDelay field, see Audio class specification.

uint8_t USB_Audio_Descriptor_StreamEndpoint_Spc_t::Subtype

Sub type value used to distinguish between audio class-specific descriptors, a value from the Audio_CSEndpoint_SubTypes_t enum.

The documentation for this struct was generated from the following file:

- Drivers/USB/Class/Common/AudioClassCommon.h