| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Pipe Control Request Management (UC3)
Pipe Control Request Management

Pipe control request management definitions for the Atmel AVR32 UC3 architecture. More...

Module for host mode request processing. This module allows for the transmission of standard, class and vendor control requests to the default control endpoint of an attached device while in host mode.

See also
  Chapter 9 of the USB 2.0 specification.