| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros
LEDs.h File Reference

Board specific LED driver header for the PJRC Teensy 1.x/2.x boards. More...

`#include "../../../../Common/Common.h"`

## Macros
#define | LEDS_ALL_LEDS LEDS_LED1
#define | LEDS_LED1 (1 << 6)
#define | LEDS_NO_LEDS 0

## Detailed Description

Note
  For version 2 Teensy boards, compile with `BOARD = TEENSY2`.

Board specific LED driver header for the PJRC Teensy boards (http://www.pjrc.com/teensy/index.html).

TEENSY:

Name | Color | Info | Active Level | Port Pin
--- | --- | --- | --- | ---
LEDS_LED1 | Green | General Indicator | High | PORTD.6

TEENSY2:

Name | Color | Info | Active Level | Port Pin
--- | --- | --- | --- | ---
LEDS_LED1 | Green | General Indicator | Low | PORTD.6

Note
  This file should not be included directly. It is automatically included as needed by the LEDs driver dispatch header located in LUFA/Drivers/Board/LEDs.h.