| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
USB_Audio_Descriptor_StreamEndpoint_Std_t Struct Reference
Common Class Definitions

Audio class-specific Streaming Endpoint Descriptor (LUFA naming conventions). More...

`#include <AudioClassCommon.h>`

## Data Fields
USB_Descriptor_Endpoint_t | Endpoint
uint8_t | Refresh
uint8_t | SyncEndpointNumber

## Detailed Description

Type define for an Audio class-specific endpoint descriptor. This contains a regular endpoint descriptor with a few Audio-class-specific extensions. See the USB Audio specification for more details.

See also
  USB_Audio_StdDescriptor_StreamEndpoint_Std_t for the version of this type with standard element names.

Note
  Regardless of CPU architecture, these values should be stored as little endian.

## Field Documentation

USB_Descriptor_Endpoint_t USB_Audio_Descriptor_StreamEndpoint_Std_t::Endpoint

Standard endpoint descriptor describing the audio endpoint.

uint8_t USB_Audio_Descriptor_StreamEndpoint_Std_t::Refresh

Always set to zero for Audio class devices.

uint8_t USB_Audio_Descriptor_StreamEndpoint_Std_t::SyncEndpointNumber

Endpoint address to send synchronization information to, if needed (zero otherwise).

The documentation for this struct was generated from the following file:

- Drivers/USB/Class/Common/AudioClassCommon.h