| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros
OLIMEXT32U4
LEDs Driver - LUFA/Drivers/Board/LEDs.h

Board specific LED driver header for the Olimex AVR-USB-T32U4. More...

## Macros
#define | LEDS_ALL_LEDS (LEDS_LED1 | LEDS_LED2 | LEDS_LED3)
#define | LEDS_LED1 (1 << 0)
#define | LEDS_LED2 (1 << 5)
#define | LEDS_LED3 (1 << 6)
#define | LEDS_NO_LEDS 0

## Detailed Description

Board specific LED driver header for the Olimex AVR-USB-T32U4 (http://www.olimex.com/dev/avr-t32u4.html).

Name | Color | Info | Active Level | Port Pin
--- | --- | --- | --- | ---
LEDS_LED1 | Yellow | RX | High | PORTB.0
LEDS_LED2 | Green | TX | High | PORTD.5
LEDS_LED3 | N/A | General Indicator (Not Mounted) | High | PORTE.6

## Macro Definition Documentation

#define LEDS_ALL_LEDS (LEDS_LED1 | LEDS_LED2 | LEDS_LED3)

LED mask for all the LEDs on the board.

#define LEDS_LED1 (1 << 0)

LED mask for the first LED on the board.

#define LEDS_LED2 (1 << 5)

LED mask for the second LED on the board.

#define LEDS_LED3 (1 << 6)

LED mask for the third LED on the board.

#define LEDS_NO_LEDS 0

LED mask for none of the board LEDs.