| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Structures | Macros | Enumerations
RNDISClassCommon.h File Reference

Common definitions and declarations for the library USB RNDIS Class driver. More...

`#include "../../Core/StdDescriptors.h"`
`#include "CDCClassCommon.h"`

## Data Structures
struct | MAC_Address_t
| MAC Address Structure. More...
struct | RNDIS_Initialize_Complete_t
| RNDIS Initialize Complete Message Structure. More...
struct | RNDIS_Initialize_Message_t
| RNDIS Initialization Message Structure. More...
struct | RNDIS_KeepAlive_Complete_t
| RNDIS Keep Alive Complete Message Structure. More...
struct | RNDIS_KeepAlive_Message_t
| RNDIS Keep Alive Message Structure. More...
struct | RNDIS_Message_Header_t
| RNDIS Common Message Header Structure. More...
struct | RNDIS_Packet_Message_t
| RNDIS Message Structure. More...
struct | RNDIS_Query_Complete_t
| RNDIS OID Property Query Complete Message Structure. More...
struct | RNDIS_Query_Message_t
| RNDIS OID Property Query Message Structure. More...
struct | RNDIS_Reset_Complete_t
| RNDIS Reset Complete Message Structure. More...
struct | RNDIS_Set_Complete_t
| RNDIS OID Property Set Complete Message Structure. More...
struct | RNDIS_Set_Message_t
| RNDIS OID Property Set Message Structure. More...

## Macros
#define | ETHERNET_FRAME_SIZE_MAX 1500
#define | REMOTE_NDIS_VERSION_MAJOR 0x01
#define | REMOTE_NDIS_VERSION_MINOR 0x00
#define | RNDIS_ERROR_LOGICAL_CMD_FAILED 0x80
#define | RNDIS_MESSAGE_BUFFER_SIZE 128
RNDIS Message Values
#define | REMOTE_NDIS_PACKET_MSG 0x00000001UL
#define | REMOTE_NDIS_INITIALIZE_MSG 0x00000002UL
#define | REMOTE_NDIS_HALT_MSG 0x00000003UL
#define | REMOTE_NDIS_QUERY_MSG 0x00000004UL
#define | REMOTE_NDIS_SET_MSG 0x00000005UL
#define | REMOTE_NDIS_RESET_MSG 0x00000006UL
#define | REMOTE_NDIS_INDICATE_STATUS_MSG 0x00000007UL
#define | REMOTE_NDIS_KEEPALIVE_MSG 0x00000008UL
RNDIS Response Values
#define | REMOTE_NDIS_INITIALIZE_CMPLT 0x80000002UL
#define | REMOTE_NDIS_QUERY_CMPLT 0x80000004UL
#define | REMOTE_NDIS_SET_CMPLT 0x80000005UL
#define | REMOTE_NDIS_RESET_CMPLT 0x80000006UL
#define | REMOTE_NDIS_KEEPALIVE_CMPLT 0x80000008UL
RNDIS Status Values
#define | REMOTE_NDIS_STATUS_SUCCESS 0x00000000UL
#define | REMOTE_NDIS_STATUS_FAILURE 0xC0000001UL
#define | REMOTE_NDIS_STATUS_INVALID_DATA 0xC0010015UL
#define | REMOTE_NDIS_STATUS_NOT_SUPPORTED 0xC00000BBUL
#define | REMOTE_NDIS_STATUS_MEDIA_CONNECT 0x4001000BUL
#define | REMOTE_NDIS_STATUS_MEDIA_DISCONNECT 0x4001000CUL
RNDIS Media States
#define | REMOTE_NDIS_MEDIA_STATE_CONNECTED 0x00000000UL
#define | REMOTE_NDIS_MEDIA_STATE_DISCONNECTED 0x00000001UL
RNDIS Media Types
#define | REMOTE_NDIS_MEDIUM_802_3 0x00000000UL
RNDIS Connection Types
#define | REMOTE_NDIS_DF_CONNECTIONLESS 0x00000001UL
#define | REMOTE_NDIS_DF_CONNECTION_ORIENTED 0x00000002UL
RNDIS Packet Types
#define | REMOTE_NDIS_PACKET_DIRECTED 0x00000001UL
#define | REMOTE_NDIS_PACKET_MULTICAST 0x00000002UL
#define | REMOTE_NDIS_PACKET_ALL_MULTICAST 0x00000004UL
#define | REMOTE_NDIS_PACKET_BROADCAST 0x00000008UL
#define | REMOTE_NDIS_PACKET_SOURCE_ROUTING 0x00000010UL
#define | REMOTE_NDIS_PACKET_PROMISCUOUS 0x00000020UL
#define | REMOTE_NDIS_PACKET_SMT 0x00000040UL
#define | REMOTE_NDIS_PACKET_ALL_LOCAL 0x00000080UL
#define | REMOTE_NDIS_PACKET_GROUP 0x00001000UL
#define | REMOTE_NDIS_PACKET_ALL_FUNCTIONAL 0x00002000UL
#define | REMOTE_NDIS_PACKET_FUNCTIONAL 0x00004000UL
#define | REMOTE_NDIS_PACKET_MAC_FRAME 0x00008000UL
RNDIS OID Values
#define | OID_GEN_SUPPORTED_LIST 0x00010101UL
#define | OID_GEN_HARDWARE_STATUS 0x00010102UL
#define | OID_GEN_MEDIA_SUPPORTED 0x00010103UL
#define | OID_GEN_MEDIA_IN_USE 0x00010104UL
#define | OID_GEN_MAXIMUM_FRAME_SIZE 0x00010106UL
#define | OID_GEN_MAXIMUM_TOTAL_SIZE 0x00010111UL
#define | OID_GEN_LINK_SPEED 0x00010107UL
#define | OID_GEN_TRANSMIT_BLOCK_SIZE 0x0001010AUL
#define | OID_GEN_RECEIVE_BLOCK_SIZE 0x0001010BUL
#define | OID_GEN_VENDOR_ID 0x0001010CUL
#define | OID_GEN_VENDOR_DESCRIPTION 0x0001010DUL
#define | OID_GEN_CURRENT_PACKET_FILTER 0x0001010EUL
#define | OID_GEN_MAXIMUM_TOTAL_SIZE 0x00010111UL
#define | OID_GEN_MEDIA_CONNECT_STATUS 0x00010114UL
#define | OID_GEN_PHYSICAL_MEDIUM 0x00010202UL
#define | OID_GEN_XMIT_OK 0x00020101UL
#define | OID_GEN_RCV_OK 0x00020102UL
#define | OID_GEN_XMIT_ERROR 0x00020103UL
#define | OID_GEN_RCV_ERROR 0x00020104UL
#define | OID_GEN_RCV_NO_BUFFER 0x00020105UL
#define | OID_802_3_PERMANENT_ADDRESS 0x01010101UL
#define | OID_802_3_CURRENT_ADDRESS 0x01010102UL
#define | OID_802_3_MULTICAST_LIST 0x01010103UL
#define | OID_802_3_MAXIMUM_LIST_SIZE 0x01010104UL
#define | OID_802_3_RCV_ERROR_ALIGNMENT 0x01020101UL
#define | OID_802_3_XMIT_ONE_COLLISION 0x01020102UL
#define | OID_802_3_XMIT_MORE_COLLISIONS 0x01020103UL

## Enumerations
enum | NDIS_Hardware_Status_t { NDIS_HardwareStatus_Ready, NDIS_HardwareStatus_Initializing, NDIS_HardwareStatus_Reset, NDIS_HardwareStatus_Closing, NDIS_HardwareStatus_NotReady }
enum | RNDIS_ClassNotifications_t { RNDIS_NOTIF_ResponseAvailable = 0x01 }
enum | RNDIS_ClassRequests_t { RNDIS_REQ_SendEncapsulatedCommand = 0x00, RNDIS_REQ_GetEncapsulatedResponse = 0x01 }
enum | RNDIS_States_t { RNDIS_Uninitialized = 0, RNDIS_Initialized = 1, RNDIS_Data_Initialized = 2 }

## Detailed Description

Common definitions and declarations for the library USB RNDIS Class driver.

Note
  This file should not be included directly. It is automatically included as needed by the USB module driver dispatch header located in LUFA/Drivers/USB.h.