| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
RNDIS_Query_Message_t Struct Reference
Common Class Definitions

RNDIS OID Property Query Message Structure. More...

`#include <RNDISClassCommon.h>`

## Data Fields
uint32_t | DeviceVcHandle
uint32_t | InformationBufferLength
uint32_t | InformationBufferOffset
uint32_t | MessageLength
uint32_t | MessageType
uint32_t | Oid
uint32_t | RequestId

## Detailed Description

Type define for a RNDIS OID Property Query command message.

Note
  Regardless of CPU architecture, these values should be stored as little endian.

## Field Documentation

uint32_t RNDIS_Query_Message_t::DeviceVcHandle

uint32_t RNDIS_Query_Message_t::InformationBufferLength

uint32_t RNDIS_Query_Message_t::InformationBufferOffset

uint32_t RNDIS_Query_Message_t::MessageLength

uint32_t RNDIS_Query_Message_t::MessageType

uint32_t RNDIS_Query_Message_t::Oid

uint32_t RNDIS_Query_Message_t::RequestId

The documentation for this struct was generated from the following file:

- Drivers/USB/Class/Common/RNDISClassCommon.h