| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Structures | Enumerations | Functions
MIDIClassHost.h File Reference

Host mode driver for the library USB MIDI Class driver. More...

`#include "../../USB.h"`
`#include "../Common/MIDIClassCommon.h"`

## Data Structures
struct | USB_ClassInfo_MIDI_Host_t
| MIDI Class Host Mode Configuration and State Structure. More...

## Enumerations
enum | MIDI_Host_EnumerationFailure_ErrorCodes_t { MIDI_ENUMERROR_NoError = 0, MIDI_ENUMERROR_InvalidConfigDescriptor = 1, MIDI_ENUMERROR_NoCompatibleInterfaceFound = 2, MIDI_ENUMERROR_PipeConfigurationFailed = 3 }

## Functions
uint8_t | MIDI_Host_ConfigurePipes (USB_ClassInfo_MIDI_Host_t *const MIDIInterfaceInfo, uint16_t ConfigDescriptorSize, void *ConfigDescriptorData) ATTR_NON_NULL_PTR_ARG(1) ATTR_NON_NULL_PTR_ARG(3)
uint8_t | MIDI_Host_Flush (USB_ClassInfo_MIDI_Host_t *const MIDIInterfaceInfo) ATTR_NON_NULL_PTR_ARG(1)
bool | MIDI_Host_ReceiveEventPacket (USB_ClassInfo_MIDI_Host_t *const MIDIInterfaceInfo, MIDI_EventPacket_t *const Event) ATTR_NON_NULL_PTR_ARG(1) ATTR_NON_NULL_PTR_ARG(2)
uint8_t | MIDI_Host_SendEventPacket (USB_ClassInfo_MIDI_Host_t *const MIDIInterfaceInfo, MIDI_EventPacket_t *const Event) ATTR_NON_NULL_PTR_ARG(1) ATTR_NON_NULL_PTR_ARG(2)
void | MIDI_Host_USBTask (USB_ClassInfo_MIDI_Host_t *const MIDIInterfaceInfo) ATTR_NON_NULL_PTR_ARG(1)

## Detailed Description

Host mode driver for the library USB MIDI Class driver.

Note
  This file should not be included directly. It is automatically included as needed by the USB module driver dispatch header located in LUFA/Drivers/USB.h.