| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Structures | Functions
PrinterClassDevice.h File Reference

Device mode driver for the library USB Printer Class driver. More...

`#include "../../USB.h"`
`#include "../Common/PrinterClassCommon.h"`
`#include <stdio.h>`

## Data Structures
struct | USB_ClassInfo_PRNT_Device_t
| Printer Class Device Mode Configuration and State Structure. More...

## Functions
void | EVENT_PRNT_Device_SoftReset (USB_ClassInfo_PRNT_Device_t *const PRNTInterfaceInfo) ATTR_NON_NULL_PTR_ARG(1)
uint16_t | PRNT_Device_BytesReceived (USB_ClassInfo_PRNT_Device_t *const PRNTInterfaceInfo) ATTR_NON_NULL_PTR_ARG(1)
bool | PRNT_Device_ConfigureEndpoints (USB_ClassInfo_PRNT_Device_t *const PRNTInterfaceInfo) ATTR_NON_NULL_PTR_ARG(1)
void | PRNT_Device_CreateBlockingStream (USB_ClassInfo_PRNT_Device_t *const PRNTInterfaceInfo, FILE *const Stream) ATTR_NON_NULL_PTR_ARG(1) ATTR_NON_NULL_PTR_ARG(2)
void | PRNT_Device_CreateStream (USB_ClassInfo_PRNT_Device_t *const PRNTInterfaceInfo, FILE *const Stream) ATTR_NON_NULL_PTR_ARG(1) ATTR_NON_NULL_PTR_ARG(2)
uint8_t | PRNT_Device_Flush (USB_ClassInfo_PRNT_Device_t *const PRNTInterfaceInfo) ATTR_NON_NULL_PTR_ARG(1)
void | PRNT_Device_ProcessControlRequest (USB_ClassInfo_PRNT_Device_t *const PRNTInterfaceInfo) ATTR_NON_NULL_PTR_ARG(1)
int16_t | PRNT_Device_ReceiveByte (USB_ClassInfo_PRNT_Device_t *const PRNTInterfaceInfo) ATTR_NON_NULL_PTR_ARG(1)
uint8_t | PRNT_Device_SendByte (USB_ClassInfo_PRNT_Device_t *const PRNTInterfaceInfo, const uint8_t Data) ATTR_NON_NULL_PTR_ARG(1)
uint8_t | PRNT_Device_SendData (USB_ClassInfo_PRNT_Device_t *const PRNTInterfaceInfo, const void *const Buffer, const uint16_t Length) ATTR_NON_NULL_PTR_ARG(1) ATTR_NON_NULL_PTR_ARG(2)
uint8_t | PRNT_Device_SendString (USB_ClassInfo_PRNT_Device_t *const PRNTInterfaceInfo, const char *const String) ATTR_NON_NULL_PTR_ARG(1) ATTR_NON_NULL_PTR_ARG(2)
void | PRNT_Device_USBTask (USB_ClassInfo_PRNT_Device_t *const PRNTInterfaceInfo) ATTR_NON_NULL_PTR_ARG(1)

## Detailed Description

Device mode driver for the library USB Printer Class driver.

Note
  This file should not be included directly. It is automatically included as needed by the USB module driver dispatch header located in LUFA/Drivers/USB.h.