| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros
EVK1100
LEDs Driver - LUFA/Drivers/Board/LEDs.h

Board specific LED driver header for the Atmel EVK1100. More...

## Macros
#define | LEDS_ALL_LEDS
#define | LEDS_LED1 (1UL << 19)
#define | LEDS_LED2 (1UL << 20)
#define | LEDS_LED3 (1UL << 21)
#define | LEDS_LED4 (1UL << 22)
#define | LEDS_LED5 (1UL << 27)
#define | LEDS_LED6 (1UL << 28)
#define | LEDS_LED7 (1UL << 29)
#define | LEDS_LED8 (1UL << 30)
#define | LEDS_NO_LEDS 0

## Detailed Description

Board specific LED driver header for the Atmel EVK1100.

Name | Color | Info | Active Level | Port Pin
--- | --- | --- | --- | ---
LEDS_LED1 | Green | LED0 LED | Low | GPIO51
LEDS_LED2 | Green | LED1 LED | Low | GPIO52
LEDS_LED3 | Green | LED2 LED | Low | GPIO53
LEDS_LED4 | Green | LED3 LED | Low | GPIO54
LEDS_LED5 | Green | LED4 LED | Low | GPIO59
LEDS_LED6 | Green | LED5 LED | Low | GPIO60
LEDS_LED7 | Green | LED6 LED | Low | GPIO61
LEDS_LED8 | Green | LED7 LED | Low | GPIO62

## Macro Definition Documentation

#define LEDS_ALL_LEDS

LED mask for all the LEDs on the board.

#define LEDS_LED1 (1UL << 19)

LED mask for the first LED on the board.

#define LEDS_LED2 (1UL << 20)

LED mask for the second LED on the board.

#define LEDS_LED3 (1UL << 21)

LED mask for the third LED on the board.

#define LEDS_LED4 (1UL << 22)

LED mask for the fourth LED on the board.

#define LEDS_LED5 (1UL << 27)

LED mask for the fifth LED on the board.

#define LEDS_LED6 (1UL << 28)

LED mask for the sixth LED on the board.

#define LEDS_LED7 (1UL << 29)

LED mask for the seventh LED on the board.

#define LEDS_LED8 (1UL << 30)

LED mask for the eighth LED on the board.

#define LEDS_NO_LEDS 0

LED mask for the none of the board LEDs