| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros
LEDs.h File Reference

Board specific LED driver header for the Atmel UC3-A3 Xplained. More...

`#include "../../../../Common/Common.h"`

## Macros
#define | LEDS_ALL_LEDS (LEDS_LED1 | LEDS_LED2 | LEDS_LED3 | LEDS_LED4 | LEDS_LED5 | LEDS_LED6)
#define | LEDS_LED1 (1UL << 3)
#define | LEDS_LED2 (1UL << 9)
#define | LEDS_LED3 (1UL << 2)
#define | LEDS_LED4 (1UL << 6)
#define | LEDS_LED5 (1UL << 18)
#define | LEDS_LED6 (1UL << 17)
#define | LEDS_NO_LEDS 0

## Detailed Description

Board specific LED driver header for the Atmel UC3-A3 Xplained.

Name | Color | Info | Active Level | Port Pin
--- | --- | --- | --- | ---
LEDS_LED1 | Yellow | LED0 LED | Low | GPIO35
LEDS_LED2 | Yellow | LED1 LED | Low | GPIO73
LEDS_LED3 | Yellow | LED2 LED | Low | GPIO34
LEDS_LED4 | Yellow | LED3 LED | Low | GPIO38
LEDS_LED5 | Green | Status | Low | GPIO50
LEDS_LED6 | Red | Power | High | GPIO49

Note
  This file should not be included directly. It is automatically included as needed by the LEDs driver dispatch header located in LUFA/Drivers/Board/LEDs.h.