| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros
LEDs.h File Reference

Board specific LED driver header for the Atmel XMEGA A3BU Xplained. More...

`#include <avr/io.h>`

## Macros
#define | LEDS_ALL_LEDS (LEDS_LED1 | LEDS_LED2 | LEDS_LED3 | LEDS_LED4)
#define | LEDS_LED1 (1 << 0)
#define | LEDS_LED2 (1 << 1)
#define | LEDS_LED3 (1 << 4)
#define | LEDS_LED4 (1 << 5)
#define | LEDS_NO_LEDS 0

## Detailed Description

Board specific LED driver header for the Atmel XMEGA A3BU Xplained.

Name | Color | Info | Active Level | Port Pin
--- | --- | --- | --- | ---
LEDS_LED1 | Yellow | LED0 LED | Low | PORTR.0
LEDS_LED2 | Yellow | LED1 LED | Low | PORTR.1
LEDS_LED3 | Red | Status Bicolour Red LED | Low | PORTD.4
LEDS_LED4 | Green | Status Bicolour Green LED | High | PORTD.5

Note
  This file should not be included directly. It is automatically included as needed by the LEDs driver dispatch header located in LUFA/Drivers/Board/LEDs.h.