| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
USB_Endpoint_Table_t Struct Reference
Endpoint Management

`#include <Endpoint.h>`

## Data Fields
uint8_t | Address
uint8_t | Banks
uint16_t | Size
uint8_t | Type

## Detailed Description

Type define for a endpoint table entry, used to configure endpoints in groups via Endpoint_ConfigureEndpointTable().

## Field Documentation

uint8_t USB_Endpoint_Table_t::Address

Address of the endpoint to configure, or zero if the table entry is to be unused.

uint8_t USB_Endpoint_Table_t::Banks

Number of hardware banks to use for the endpoint.

uint16_t USB_Endpoint_Table_t::Size

Size of the endpoint bank, in bytes.

uint8_t USB_Endpoint_Table_t::Type

Type of the endpoint, a `EP_TYPE_*` mask.

The documentation for this struct was generated from the following file:

- Drivers/USB/Core/Endpoint.h