| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Atmel USB XMEGA AVR (XMEGA)

Warning
  The XMEGA device support is currently experimental (incomplete and/or non-functional), and is included for preview purposes only.

# Supported Microcontroller Models

Currently supported XMEGA models:

Part | USB Device Mode | USB Host Mode
--- | --- | ---
ATXMEGA16A4U | Yes | No
ATXMEGA32A4U | Yes | No
ATXMEGA64A4U | Yes | No
ATXMEGA128A4U | Yes | No
ATXMEGA64A3U | Yes | No
ATXMEGA128A3U | Yes | No
ATXMEGA192A3U | Yes | No
ATXMEGA256A3U | Yes | No
ATXMEGA256A3BU | Yes | No
ATXMEGA128A1U | Yes | No
ATXMEGA64B3 | Yes | No
ATXMEGA128B3 | Yes | No
ATXMEGA64B1 | Yes | No
ATXMEGA128B1 | Yes | No
ATXMEGA64C3 | Yes | No
ATXMEGA128C3 | Yes | No
ATXMEGA192C3 | Yes | No
ATXMEGA256C3 | Yes | No
ATXMEGA384C3 | Yes | No
ATXMEGA16C4 | Yes | No
ATXMEGA32C4 | Yes | No

# Supported Atmel Boards

Currently supported Atmel XMEGA boards (see Board Types):

- XMEGA A3BU Xplained
- XMEGA B1 Xplained
- XMEGA C3 Xplained

# Supported Third Party Boards

Currently supported third-party boards (see Board Types for makefile `BOARD` constant names):

- Custom User Boards (with Board Drivers if desired, see Writing LUFA Board Drivers)