| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Enumerations | Variables
DeviceStandardReq.h File Reference

USB device standard request management. More...

`#include "../../../Common/Common.h"`
`#include "USBMode.h"`
`#include "StdDescriptors.h"`
`#include "Events.h"`
`#include "StdRequestType.h"`
`#include "USBTask.h"`
`#include "USBController.h"`

## Enumerations
enum | USB_DescriptorMemorySpaces_t { MEMSPACE_FLASH = 0, MEMSPACE_EEPROM = 1, MEMSPACE_RAM = 2 }

## Variables
uint8_t | USB_Device_ConfigurationNumber
bool | USB_Device_CurrentlySelfPowered
bool | USB_Device_RemoteWakeupEnabled

## Detailed Description

This file contains the function prototypes necessary for the processing of incoming standard control requests when the library is in USB device mode.

Note
  This file should not be included directly. It is automatically included as needed by the USB driver dispatch header located in LUFA/Drivers/USB/USB.h.