| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros
LEDs.h File Reference

Board specific LED driver header for the Atmel USBKEY. More...

`#include "../../../../Common/Common.h"`

## Macros
#define | LEDS_ALL_LEDS (LEDS_LED1 | LEDS_LED2 | LEDS_LED3 | LEDS_LED4)
#define | LEDS_LED1 (1 << 4)
#define | LEDS_LED2 (1 << 5)
#define | LEDS_LED3 (1 << 7)
#define | LEDS_LED4 (1 << 6)
#define | LEDS_NO_LEDS 0

## Detailed Description

Board specific LED driver header for the Atmel USBKEY.

Name | Color | Info | Active Level | Port Pin
--- | --- | --- | --- | ---
LEDS_LED1 | Red | Bicolor Indicator 1 | High | PORTD.4
LEDS_LED2 | Green | Bicolor Indicator 1 | High | PORTD.5
LEDS_LED3 | Red | Bicolor Indicator 2 | High | PORTD.6
LEDS_LED4 | Green | Bicolor Indicator 2 | High | PORTD.7

Note
  This file should not be included directly. It is automatically included as needed by the LEDs driver dispatch header located in LUFA/Drivers/Board/LEDs.h.