| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
USB_KeyboardReport_Data_t Struct Reference
Common Class Definitions

Standard HID Boot Protocol Keyboard Report. More...

`#include <HIDClassCommon.h>`

## Data Fields
uint8_t | KeyCode [6]
uint8_t | Modifier
uint8_t | Reserved

## Detailed Description

Type define for a standard Boot Protocol Keyboard report

## Field Documentation

uint8_t USB_KeyboardReport_Data_t::KeyCode[6]

Key codes of the currently pressed keys.

uint8_t USB_KeyboardReport_Data_t::Modifier

Keyboard modifier byte, indicating pressed modifier keys (a combination of `HID_KEYBOARD_MODIFER_*` masks).

uint8_t USB_KeyboardReport_Data_t::Reserved

Reserved for OEM use, always set to 0.

The documentation for this struct was generated from the following file:

- Drivers/USB/Class/Common/HIDClassCommon.h