| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Atmel 32-Bit UC3 AVR (UC3)

Warning
  The AVR32 UC3 device support is currently experimental, and is included for preview purposes only.

# Supported Microcontroller Models

Currently supported UC3 models:

Part | USB Device Mode | USB Host Mode
--- | --- | ---
AT32UC3A364 | Yes | Yes
AT32UC3A364S | Yes | Yes
AT32UC3A464 | Yes | Yes
AT32UC3A464S | Yes | Yes
AT32UC3B064 | Yes | Yes
AT32UC3B164 | Yes | Yes
AT32UC3A0128 | Yes | Yes
AT32UC3A1128 | Yes | Yes
AT32UC3A3128 | Yes | Yes
AT32UC3A3128S | Yes | Yes
AT32UC3A4128 | Yes | Yes
AT32UC3A4128S | Yes | Yes
AT32UC3B0128 | Yes | Yes
AT32UC3B1128 | Yes | Yes
AT32UC3A0256 | Yes | Yes
AT32UC3A1256 | Yes | Yes
AT32UC3A3256 | Yes | Yes
AT32UC3A3256S | Yes | Yes
AT32UC3A4256 | Yes | Yes
AT32UC3A4256S | Yes | Yes
AT32UC3B0256 | Yes | Yes
AT32UC3B1256 | Yes | Yes
AT32UC3A0512 | Yes | Yes
AT32UC3A1512 | Yes | Yes
AT32UC3B0512 | Yes | Yes
AT32UC3B1512 | Yes | Yes

# Supported Atmel Boards

Currently supported Atmel UC3 boards (see Board Types):

- EVK1100
- EVK1101
- EVK1104
- UC3-A3 Xplained

# Supported Third Party Boards

Currently supported third-party boards (see Board Types for makefile `BOARD` constant names):

- Custom User Boards (with Board Drivers if desired, see Writing LUFA Board Drivers)