| LUFA Library 140302 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
USB_Pipe_Table_t Struct Reference
Pipe Management

`#include <Pipe.h>`

## Data Fields
uint8_t | Address
uint8_t | Banks
uint8_t | EndpointAddress
uint16_t | Size
uint8_t | Type

## Detailed Description

Type define for a pipe table entry, used to configure pipes in groups via Pipe_ConfigurePipeTable().

## Field Documentation

uint8_t USB_Pipe_Table_t::Address

Address of the pipe to configure, or zero if the table entry is to be unused.

uint8_t USB_Pipe_Table_t::Banks

Number of hardware banks to use for the pipe.

uint8_t USB_Pipe_Table_t::EndpointAddress

Address of the endpoint in the connected device.

uint16_t USB_Pipe_Table_t::Size

Size of the pipe bank, in bytes.

uint8_t USB_Pipe_Table_t::Type

Type of the endpoint, a `EP_TYPE_*` mask.

The documentation for this struct was generated from the following file:

- Drivers/USB/Core/Pipe.h